
USGS Gage vs VAHydro Model


09/11/2023

# Appendix X - Model Calibration Analysis:


## Flow Duration Curve Plot:




## L90 Model Performance Bar Plot:




## L30 Model Performance Bar Plot:




## L7 Model Performance Bar Plot:





## L1 Model Performance Bar Plot:




## Model Performance Scatterplots:









## Metrics Table:

| stat | gage | gage\_year | model | model\_year |
| --- | --- | --- | --- | --- |
| l90 | 472.28 | 1999 | 409.82 | 1999 |
| l30 | 353.59 | 1999 | 229.59 | 1992 |
| l7 | 272.67 | 1999 | 214.4 | 1992 |
| l1 | 252.2 | 1999 | 209.08 | 2002 |